{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["安装","苗木","土建"],"read":"whole","date_system":"1900"}

{"sheet":"安装","index":0,"n_rows":25,"n_cols":9,"rows_kept":25,"merged":[[0,0,1,8],[2,0,2,8],[3,0,5,0],[3,1,5,1],[3,2,5,2],[3,3,5,3],[3,4,5,4],[3,5,5,5],[3,6,3,8],[4,6,5,6],[4,7,5,7],[6,2,6,3],[15,2,15,3],[19,2,19,3],[20,2,20,3],[24,0,24,6]]}
["分部分项工程和单价措施项目清单与计价表"]
[]
["工程名称:秀逸苏杭30#31#室外景观-安装部分     标段:"]
["序号","项目编码","项目名称","项目特征\r\n描述","计量\r\n单位","工程量","金   额（元）"]
[{"$nulls":6},"综合\r\n单价","合价","其中"]
[{"$nulls":8},"暂估价"]
[null,null,"一、电气工程"]
[1,"030412007001","景观灯","1、包括基础浇筑(包括土石方),立灯杆及杆座安装；\n2、灯架安装；\n3、焊压接线端子；\n4、铁构件制作、安装,除锈、刷油；\n5、灯杆编号,接地；\n6、包括设计及规范要求的全部工作内容","套",{"v":4,"d":"4.000"}]
[2,"030412004002","射树灯","1、包括基础浇筑(包括土石方)；\n2、包括本体及支架制作、安装,除锈、刷油；\n3、接地；\n4、包括设计及规范要求的全部工作内容","套",{"v":2,"d":"2.000"}]
[3,"030412004005","壁灯         ","1、包括本体及支架制作、安装,除锈、刷油；\n2、接地；\n3、包括设计及规范要求的全部工作内容","套",{"v":4,"d":"4.000"}]
[4,"030412007002","庭院灯         ","1、包括基础浇筑(包括土石方),立灯杆及杆座安装；\n2、灯架安装；\n3、焊压接线端子；\n4、铁构件制作、安装,除锈、刷油；\n5、灯杆编号,接地；\n6、包括设计及规范要求的全部工作内容","套",{"v":11,"d":"11.000"}]
[5,"030408001001","电力电缆 YJV  4*2.5 PE32 FC","1、开挖电缆沟、揭(盖)盖板、回填；\n2、电缆敷设,电缆头制作、安装；\n3、过路保护管敷设；\n4、防火堵洞,电缆防护,电缆防火隔板,电缆防火涂料；\n5、包括设计及规范要求的全部工作内容","m",{"v":6,"d":"6.000"}]
[6,"030408001002","电力电缆YJV  4*6 PE50 FC","1、开挖电缆沟、揭(盖)盖板、回填；\n2、电缆敷设,电缆头制作、安装；\n3、过路保护管敷设；\n4、防火堵洞,电缆防护,电缆防火隔板,电缆防火涂料；\n5、包括设计及规范要求的全部工作内容","m",{"v":40,"d":"40.000"}]
[7,"030408001003","电力电缆 YJV  3*4 PE32 FC","1、开挖电缆沟、揭(盖)盖板、回填；\n2、电缆敷设,电缆头制作、安装；\n3、过路保护管敷设；\n4、防火堵洞,电缆防护,电缆防火隔板,电缆防火涂料；\n5、包括设计及规范要求的全部工作内容","m",{"v":300,"d":"300.000"}]
[8,"030408001004","电力电缆 YJV  3*2.5 PE32 FC","1、开挖电缆沟、揭(盖)盖板、回填；\n2、电缆敷设,电缆头制作、安装；\n3、过路保护管敷设；\n4、防火堵洞,电缆防护,电缆防火隔板,电缆防火涂料；\n5、包括设计及规范要求的全部工作内容","m",{"v":300,"d":"300.000"}]
[9,null,"二、给水工程"]
[10,"031001006001","PE给水管DE50","1、包括管道、管件及弯管的制作、安装；\n2、包括套管及防水套管制作、安装；\n3、给水管道消毒、冲洗,水压试验；\n4、包括挖、填土。\n5、包括设计及规范要求的全部工作内容","m",{"v":250,"d":"250.000"}]
[11,"031001002001","过路保护钢管DN80","1、包括管道、管件及弯管的制作、安装；\n2、包括挖、填土及混凝土地面开挖回填；\n3、包括设计及规范要求的全部工作内容。","m",{"v":20,"d":"20.000"}]
[12,"031003001001","快速给水器  DN25","1、包括阀门购置安装；\n2、包括设计及规范要求的全部工作内容","个",{"v":8,"d":"8.000"}]
[13,null,"分部小计"]
[14,null,"三、土建部分"]
[15,"010401011001","手控井","1、包括井砌筑、粉刷；\n2、包括挖、填土；\n3、包括设计及规范要求的全部工作内容。","座",{"v":1,"d":"1.000"}]
[16,"010401011002","阀门井（600*400）","1、包括井砌筑、粉刷；\n2、包括挖、填土；\n3、包括设计及规范要求的全部工作内容。","座",{"v":1,"d":"1.000"}]
[17,"070205001001","不锈钢隐形井盖","1、包括本体及支架制作、安装,除锈、刷油；(600*600)\n2、包括设计及规范要求的全部工作内容","块",{"v":1,"d":"1.000"}]
["合   计"]

{"sheet":"苗木","index":1,"n_rows":35,"n_cols":10,"rows_kept":35,"merged":[[0,0,0,9],[1,0,1,9],[2,0,3,0],[2,1,3,1],[2,2,2,4],[2,5,3,5],[2,6,3,6],[2,7,3,7],[2,8,3,8],[2,9,3,9],[34,1,34,7]]}
["秀逸苏杭30#31#景观-绿化部分"]
["工程量清单报价表"]
["序 号","名   称","规格（cm)",null,null,"数 量","单 位","综合单价\n","综合合价","备  注"]
[null,null,"高度（cm)","蓬径（cm)","胸/地径（cm)"]
[1,"高杆女贞A",null,"180-250","10-11.9",1,"株",null,null,"全冠、树形优美"]
[3,"高杆女贞C",null,null,"18-19.9",1,"株",null,null,"全冠、树形优美"]
[6,"朴树B",null,null,"20-21.9",3,"株",null,null,"移栽苗、全冠、树形优美"]
[9,"榉树",null,null,"14-15.9",10,"株",null,null,"树干直、树形优美、飘逸"]
[12,"白玉兰A",null,null,"D7-8",1,"株",null,null,"造型优美，带骨架，全冠"]
[16,"本石楠",null,"300-320",null,9,"株",null,null,"造型优美，体形丰满"]
[18,"红叶石楠树A",null,"250-280",null,5,"株",null,null,"造型优美，体形丰满"]
[19,"红叶石楠树B",null,"200-230",null,17,"株",null,null,"造型优美，体形丰满"]
[20,"鸡爪槭A",null,null,"D7-8",3,"株",null,null,"造型优美，体形丰满"]
[22,"日本晚樱A",null,null,"D5-6",11,"株",null,null,"造型优美，体形丰满"]
[23,"苏铁",null,"100-120",null,2,"株",null,null,"造型优美，分枝饱满"]
[24,"红枫",null,null,"D5-6",4,"株",null,null,"造型优美，带骨架"]
[26,"红梅",null,null,"D5-6",8,"株",null,null,"造型优美，带骨架"]
[28,"西府海棠",null,null,"D5-6",2,"株",null,null,"造型优美"]
[31,"金镶玉竹",350,null,null,15,"m²",null,null,"造型优美，修剪整齐，高度统一,16株/m²"]
[33,"红叶石楠球A",null,"180-209",null,6,"株",null,null,"造型优美，球型饱满"]
[34,"红叶石楠球B",null,"150-179",null,10,"株",null,null,"造型优美，球型饱满"]
[35,"大叶黄杨球",null,"140-159",null,18,"株",null,null,"造型优美，球型饱满"]
[36,"变色女贞球",null,"120-139",null,8,"株",null,null,"造型优美，球型饱满"]
[37,"银姬小蜡球",null,"120-139",null,7,"株",null,null,"造型优美，球型饱满"]
[39,"红叶石楠","25-30","20-30",null,{"$f":"30+37+18+27","v":112},"m²",null,null,"64株/m²"]
[40,"金边黄杨","30-40",null,null,{"$f":"33+59+54+10","v":156},"m²",null,null,"121株/m²"]
[41,"金森女贞","25-30","20-30",null,{"$f":"84+11+88+65","v":248},"m²",null,null,"64株/m²"]
[42,"海桐","25-30",null,null,{"$f":"83+38+18+57","v":196},"m²",null,null,"49株/m²"]
[43,"红王子锦带","40-45",null,null,{"$f":"44+21","v":65},"m²",null,null,"64株/m²"]
[44,"品种月季","35-40",null,null,24,"m²",null,null,"36株/m²"]
[45,"红帽子月季","35-40",null,null,4,"m²",null,null,"49株/m²"]
[46,"常夏石竹",{"$nulls":3},35,"m²",null,null,"81株/m²"]
[47,"时令花卉",{"$nulls":3},81,"m²",null,null,"49株/m²"]
[49,"绿地平整",{"$nulls":3},930,"m²"]
[50,"合    计"]

{"sheet":"土建","index":2,"n_rows":46,"n_cols":9,"rows_kept":46,"merged":[[0,0,1,8],[2,0,2,8],[3,0,5,0],[3,1,5,1],[3,2,5,2],[3,3,5,3],[3,4,5,4],[3,5,5,5],[3,6,3,8],[4,6,5,6],[4,7,5,7],[6,2,6,3],[10,2,10,3],[11,2,11,3],[15,2,15,3],[16,2,16,3],[20,2,20,3],[21,2,21,3],[29,2,29,3],[30,2,30,3],[35,2,35,3],[36,2,36,3],[41,2,41,3],[42,2,42,3],[44,2,44,3],[45,0,45,6]]}
["分部分项工程和单价措施项目清单与计价表"]
[]
["工程名称:秀逸苏杭30#31#景观-土建部分     标段:"]
["序号","项目编码","项目名称","项目特征\r\n描述","计量\r\n单位","工程量","金   额（元）"]
[{"$nulls":6},"综合\r\n单价","合价","其中"]
[{"$nulls":8},"暂估价"]
[null,null,"一、土方工程"]
["1","010101003001","挖沟槽土方","1、土壤类别:一、二类土\n2、挖土深度:详设计图纸 \n3、弃土运距:运距自行考虑","m3",{"v":45,"d":"45.000"}]
["2","040103001001","回填方","1、密实度要求:符合设计及规范要求\n2、填方材料品种:素土 \n3、填方来源、运距:自行考虑","m3",{"v":12400,"d":"12400.000"}]
["3","040103001002","绿化种植土方","1、密实度要求:符合设计及规范要求\n2、填方材料品种:60%素土 ，40%营养土\n3、填方来源、运距:自行考虑\n","m3",{"v":1300,"d":"1300.000"}]
[null,null,"分部小计"]
[null,null,"二、车行广场铺地"]
["4","010201001001","路基垫层","\n1、碎石垫层200厚\n","m3",{"v":535,"d":"535.000"}]
["4","010201001001","路基垫层","1、素砼垫层120厚C20\n2、素土分层夯实，压实系数>=0.94\n；其它未详之处详见图纸设计","m3",{"v":321,"d":"321.000"}]
["6","011102001002","石材楼地面","1、结合层厚度、砂浆配合比:30厚1:3干硬性水泥砂浆\n\n2、面层材料品种、规格、颜色:五莲红花岗岩荔枝面 600*600*50","m2",{"v":2677,"d":"2677.000"}]
[null,null,"分部小计"]
[null,null,"三、车行沥青铺地"]
["4","010201001001","路基垫层","\n1、碎石垫层120厚\n","m3",{"v":232,"d":"232.000"}]
["4","010201001001","路基垫层","1、素砼垫层120厚C20\n2、素土分层夯实，压实系数>=0.94\n；其它未详之处详见图纸设计","m3",{"v":232,"d":"232.000"}]
["13","040203006001","沥青混凝土","1、 AC-13C 细粒式沥青砼\n2、厚度: 8cm厚","m2",{"v":1935,"d":"1935.000"}]
[null,null,"分部小计"]
[null,null,"四、人行铺地"]
["4","010201001001","路基垫层","\n1、碎石垫层200厚\n","m3",{"v":57.63,"d":"57.630"}]
["4","010201001001","路基垫层","1、素砼垫层120厚C20\n2、素土分层夯实，压实系数>=0.94\n；其它未详之处详见图纸设计","m3",{"v":34.58,"d":"34.580"}]
["16","050201001002","园路铺地","1、结合层厚度、砂浆配合比:30厚1:3干硬性水泥砂浆\n\n2、面层材料品种、规格、颜色:芝麻白花岗岩荔枝面 300*300*30\n","m2",{"v":50.8,"d":"50.800"}]
["17","050201001003","园路筑边","1、结合层厚度、砂浆配合比:30厚1:3干硬性水泥砂浆\n\n2、面层材料品种、规格、颜色:灰麻花岗岩火烧面 600*200*50\n","m2",{"v":12.4,"d":"12.400"}]
["18","050201001004","园路铺地","1、结合层厚度、砂浆配合比:30厚1:3干硬性水泥砂浆\n\n2、面层材料品种、规格、颜色:芝麻白烧面 200*100*20\n","m2",{"v":24.64,"d":"24.640"}]
["19","050201001005","园路铺地","1、结合层厚度、砂浆配合比:30厚1:3干硬性水泥砂浆\n\n2、面层材料品种、规格、颜色:芝麻白花岗岩荔枝面 300*300*30\n","m2",{"v":50.8,"d":"50.800"}]
["20","050201001006","园路筑边","1、结合层厚度、砂浆配合比:30厚1:3干硬性水泥砂浆\n\n2、面层材料品种、规格、颜色:灰麻花岗岩烧面 600*200*30","m2",{"v":18.4,"d":"18.400"}]
[null,null,"分部小计"]
[null,null,"五、停车位"]
["4","010201001001","路基垫层","\n1、碎石垫层200厚\n","m3",{"v":98,"d":"98.000"}]
["4","010201001001","路基垫层","1、素砼垫层120厚C20\n2、素土分层夯实，压实系数>=0.94\n；其它未详之处详见图纸设计","m3",{"v":58.8,"d":"58.800"}]
["28","050201001011","园路铺地","1、结合层厚度、砂浆配合比:30厚1:3干硬性水泥砂浆\n\n2、面层材料品种、规格、颜色:灰麻花岗岩火烧面 600*200*50\n","m2",{"v":65.32,"d":"65.320"}]
["29","050201005002","嵌草砖(格)铺装","1、结合层厚度、砂浆配合比:30厚1:3干硬性水泥砂浆\n\n2、面层材料品种、规格、颜色:绿色植草砖 250*190*60\n3、每平方铺0.05立方营养土，每平方草籽30g.","m2",{"v":178.68,"d":"178.680"}]
[null,null,"分部小计"]
[null,null,"六、侧石路沿"]
["32","050201003003","路牙铺设","1、五莲红火烧面平石 600*300*50\n2、30厚1:3干硬性水泥砂浆\n3、素土分层夯实，压实系数>=0.94\n","m",{"v":315,"d":"315.000"}]
["33","050201003004","路牙铺设","1、五莲红火烧面平石 600*300*50 （弧形加工） \n2、30厚1:3干硬性水泥砂浆\n3、素土分层夯实，压实系数>=0.94\n","m",{"v":36,"d":"36.000"}]
["34","050201003005","路牙铺设","1、五莲红火烧面侧石  600*200*200\n2、30厚1:3干硬性水泥砂浆\n3、素土分层夯实，压实系数>=0.94\n","m",{"v":390,"d":"390.000"}]
["35","050201003006","路牙铺设","1、五莲红火烧面侧石  600*200*200 （弧形加工） \n2、30厚1:3干硬性水泥砂浆\n3、素土分层夯实，压实系数>=0.94\n","m",{"v":60,"d":"60.000"}]
[null,null,"分部小计"]
[null,null,"七、其它园建"]
["53","050307011001","门卫（LD1.05）","1、内外装饰面\n2、屋面防水\n3、主体结构含模板\n4、基础垫层\n；其它未详之处详见图纸设计","座",{"v":1,"d":"1.000"}]
[null,null,"分部小计"]
["合   计"]